Wireless control Solexa Home

Wireless control for the automatic and manual control of sunshades, windows, lighting and heating. Set with weather station, wireless control unit with touch display and base station. Wireless connection of the participants via Elsner RF.
The weather station records brightness (1 sun sensor), wind speed, precipitation and temperature and determines date, time and installation coordinates for the sun position calculation via an integrated GPS receiver. It controls a directly connected 230 V drive via an integrated motor control unit and integrates up to 16 Elsner RF wireless actuators and up to 32 Elsner RF operating devices/sensors.
Manual operation via the touch display of the wireless control unit, via the Solexa Mobile App and via an Elsner wireless remote control.
Automatic control based on time, indoor temperature, outdoor temperature, brightness, sun position, wind speed and precipitation:
-	Shading automatic for shutters, awnings and blinds according to the brightness, with direction of the sun, movement delays, indoor and outdoor temperature blocks, wind, rain and frost alarm, movement and slat position, night and timed closing as well as timed opening
-	Ventilation automatic for casement and sliding windows according to the indoor temperature, with outdoor temperature block, wind, rain and frost alarm, stepped opening position and timer functions
-	Light automatic according to the outdoor brightness (day/night) and time, with dim level when using dimming modules
-	Heating automatic for one or two level heating according to the indoor temperature, with day/night (timer switch) and a timer switch for manual heating
-	Roof gutter automatic for switching a heating within a defined outdoor temperature range
For all outputs, a daily automatic reset and an automatic reset after manual operation can be set.
Wireless Elsner RF 868.0...868.6 MHz, transmission power ≤ 25 mW. WLAN 2400...2483.5 MHz, transmission power ≤ 100 mW, for connecting the Solexa Mobile App. Wireless control unit with permanently integrated battery.
Weather station: degree of protection IP44. Voltage 110 V AC/60 Hz or 230 V AC/50 Hz. Power consumption ≤ 2.5 W. Drive output for 1 drive, max. motor load 500 VA (230 V). Dimensions approx. 96 × 100 × 128 (W x H x D in mm). Surface-mounted or pole installation. Colour white/translucent.
Control unit: degree of protection IP20. Touch display, visible diagonal 126 mm. Dimensions approx. 143 × 96 × 14 (W x H x D in mm). Colour white.
Base station: degree of protection IP20. Power supply via USB charger (output 5 V DC). WLAN connection for the Solexa Mobile App. Indoor temperature sensor. Dimensions approx. 143 × 99 × 60 (W x H x D in mm). Colour white.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 10156 Solexa Home