Interference filter SF-ST

Interference filter for motors. Reduction of electromagnetic interference pulses by means of integrated capacitors and resistors to avoid malfunctions of adjacent electronics.
Installation between load and supply line. Connection exclusively via STAK/STAS connectors on flexible cables, locking of the connectors with securing brackets.
Vibration-free installation, without permanent direct sunlight (plastic housing, not UV-resistant). Degree of protection IP54.
Rated voltage 230 V AC, rated current 16 A. Overvoltage category III, pollution degree 2.
Dimensions approx. 149 x 37 x 26 (W x H x D in mm, without securing brackets).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 20401 SF-ST