Combined indoor sensor WGTH gl for WS1/WS1000, white

Additional sensor for indoor temperature and humidity for building controls WS1 Color/Style, (KNX) WS1000 Color/Style/Connect. With Solexa II control, only the temperature for the automatic system is evaluated.
Radio communication, frequency 868.2 MHz, Elsner RF. Operating voltage: 7...30 V DC.
Wall installation, flush-mounted in equipment socket. Supplied with frame. Dimensions plastic housing: approx. 55 x 55 (W x H in mm), installation depth approx. 8 mm. Base plate dimensions: approx. 71 x 71 (W x H in mm). Colour white.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 20557 WGTH gl, white