WS1 STYLE WITHOUT DRIVE OUTPUTS:

WS1 Style-0 control system invitation to tender

Central unit with integrated indoor sensor (for temperature and air humidity) and weather station (with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver). 2 multi-function outputs (for heating, cooling, ventilation unit, alarm, roof gutter  heating, light, dimmer). 2 multi-function inputs (for motion detectors, smoke alarms, closed contact, status message for a separate air conditioning system, automatic functions reset). 32 free wireless channels (for devices with Elsner radio RF, e.g. exhaust air extraction units, relays, motor control units, fan modules, indoor sensors, key interface, remote control). 
Manual control for the connected drives/units via 5.7-inch real glass touch display. Connections for 4 local wall push buttons.
Central unit dimensions 181 x 131 x 8 (W x H x installation depth in mm), flush or cavity wall mounting, dimensions of flush mounting box 172 x 122 x 81 (W x H x D in mm). Weather station dimensions 62 x 71 x 152 (W x H x D in mm). 
Available in white/grey or dark grey/black.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: WS1 Style-0

WS1 STYLE WITH 230 V DRIVE OUTPUTS:

WS1 Style-1 control system invitation to tender

Central unit with integrated indoor sensor (for temperature and air humidity) and weather station (with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver). 1 drive output 230 V (for blinds, shutters, roller shutters, windows, sliding door), 2 multi-function outputs (for heating, cooling, ventilation unit, alarm, roof gutter heating, lighting, dimmer). 2 multi-function inputs (for motion detectors, smoke alarms, closed contact, status message for a separate air conditioning system, automatic functions reset). 32 free wireless channels (for devices with Elsner radio RF, e.g. exhaust air extraction units, relays, motor control units, fan modules, indoor sensors, key interface, remote control). 
Manual control for the connected drives/units via 5.7-inch real glass touch display. Connections for 4 local wall push buttons.
Central unit dimensions 181 x 131 x 8 (W x H x installation depth in mm), flush or cavity wall mounting, dimensions of flush mounting box 172 x 122 x 81 (W x H x D in mm). Weather station dimensions 62 x 71 x 152 (W x H x D in mm). 
Available in white/grey or dark grey/black.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: WS1 Style-1

WS1 Style-2 control system invitation to tender

Central unit with integrated indoor sensor (for temperature and air humidity) and weather station (with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver). 2 drive output 230 V (for blinds, shutters, roller shutters, windows, sliding door), 2 multi-function outputs (for heating, cooling, ventilation unit, alarm, roof gutter heating, lighting, dimmer). 2 multi-function inputs (for motion detectors, smoke alarms, closed contact, status message for a separate air conditioning system, automatic functions reset). 32 free wireless channels (for devices with Elsner radio RF, e.g. exhaust air extraction units, relays, motor control units, fan modules, indoor sensors, key interface, remote control). 
Manual control for the connected drives/units via 5.7-inch real glass touch display. Connections for 4 local wall push buttons.
Central unit dimensions 181 x 131 x 8 (W x H x installation depth in mm), flush or cavity wall mounting, dimensions of flush mounting box 172 x 122 x 81 (W x H x D in mm). Weather station dimensions 62 x 71 x 152 (W x H x D in mm). 
Available in white/grey or dark grey/black.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: WS1 Style-2

WS1 Style-3 control system invitation to tender

Central unit with integrated indoor sensor (for temperature and air humidity) and weather station (with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver). 3 drive output 230 V (for blinds, shutters, roller shutters, windows, sliding door), 2 multi-function outputs (for heating, cooling, ventilation unit, alarm, roof gutter heating, lighting, dimmer). 2 multi-function inputs (for motion detectors, smoke alarms, closed contact, status message for a separate air conditioning system, automatic functions reset). 32 free wireless channels (for devices with Elsner radio RF, e.g. exhaust air extraction units, relays, motor control units, fan modules, indoor sensors, key interface, remote control). 
Manual control for the connected drives/units via 5.7-inch real glass touch display. Connections for 4 local wall push buttons.
Central unit dimensions 181 x 131 x 8 (W x H x installation depth in mm), flush or cavity wall mounting, dimensions of flush mounting box 172 x 122 x 81 (W x H x D in mm). Weather station dimensions 62 x 71 x 152 (W x H x D in mm). 
Available in white/grey or dark grey/black.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: WS1 Style-3

WS1 Style-4 control system invitation to tender

Central unit with integrated indoor sensor (for temperature and air humidity) and weather station (with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver). 4 drive output 230 V (for blinds, shutters, roller shutters, windows, sliding door), 2 multi-function outputs (for heating, cooling, ventilation unit, alarm, roof gutter heating, lighting, dimmer). 2 multi-function inputs (for motion detectors, smoke alarms, closed contact, status message for a separate air conditioning system, automatic functions reset). 32 free wireless channels (for devices with Elsner radio RF, e.g. exhaust air extraction units, relays, motor control units, fan modules, indoor sensors, key interface, remote control). 
Manual control for the connected drives/units via 5.7-inch real glass touch display. Connections for 4 local wall push buttons.
Central unit dimensions 181 x 131 x 8 (W x H x installation depth in mm), flush or cavity wall mounting, dimensions of flush mounting box 172 x 122 x 81 (W x H x D in mm). Weather station dimensions 62 x 71 x 152 (W x H x D in mm). 
Available in white/grey or dark grey/black.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: WS1 Style-4

WS1 STYLE WITH DRIVE OUTPUTS FREE OF POTENTIAL:

WS1 Style-4 PF control system invitation to tender

Central unit with integrated indoor sensor (for temperature and air humidity) and weather station (with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver). 4 drive outputs free of potential (for blinds, shutters, roller shutters, windows, sliding door), 2 multi-function outputs (for heating, cooling, ventilation unit, alarm, roof gutter heating, lighting, dimmer). 2 multi-function inputs (for motion detectors, smoke alarms, closed contact, status message for a separate air conditioning system, automatic functions reset). 32 free wireless channels (for devices with Elsner radio RF, e.g. exhaust air extraction units, relays, motor control units, fan modules, indoor sensors, key interface, remote control). 
Manual control for the connected drives/units via 5.7-inch real glass touch display. Connections for 4 local wall push buttons.
Central unit dimensions 181 x 131 x 8 (W x H x installation depth in mm), flush or cavity wall mounting, dimensions of flush mounting box 172 x 122 x 81 (W x H x D in mm). Weather station dimensions 62 x 71 x 152 (W x H x D in mm). 
Colour: white/grey.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: WS1 Style-4 PF

REMOTE CONTROL FOR WS1 STYLE:

Remo 8 wireless remote control invitation to tender

Hand-held transmitter with 8 channels. Up/Down/Stop keys, display for channel indication. With magnetic wall bracket.
Hand-held transmitter dimensions 41 x 140 x 21 (W x H x D in mm). Wall bracket dimensions 54 x 150 x 11 (W x H x D in mm).
Available in white/grey or aluminium/graphite.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: Remo 8