Radio remote control Remo 8i

Radio remote control with 8 channels for Elsner controllers and control units that communicate via the Elsner RF radio protocol. Operation of drives and loads with up/down/stop or on/off. One or more radio channels can be controlled with each channel.
Operation via 5 navigation buttons. Display showing the channel name. Settings via a menu on the device:
-	Teach-in and deletion of the radio connections per channel
-	Channel name freely definable, two lines (2 × 16 characters), with upper and lower case letters, numbers and special characters
-	Font size of the channel name switchable (normal/large)
-	Direction of rotation switchable per channel (normal/inverse)
-	Individual channels can be hidden for operation
-	Cloning: settings including the radio connections can be transferred to further Remo 8i
-	Menu language German, English, Spanish, French or Italian
-	Reset to factory settings, display of the device information
Housing plastic. Wall-mounted holder with screw cover included in delivery. Ambient temperature 0...+45 °C at 0...95 % RH (non-condensing), storage temperature -10...+50 °C. Radio Elsner RF 868.0...868.6 MHz, transmission power ≤ 25 mW. Voltage 2 × 1.5 V, alkaline-manganese AAA/Micro (LR03), non-rechargeable; rechargeable batteries are not permitted. Batteries included. Dimensions transmitter 44 × 172 × 22 (W x H x D in mm), dimensions holder 49 × 52 × 31 (W x H x D in mm).
Colour: black.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 60521 Remo 8i