Wireless dimmer RF-L LED-ST IP53

Wireless dimmer for 1 consumer for controllers WS1000 Colour, KNX WS1000 Colour, WS1 Colour, WS1000 Style, KNX WS1000 Style, WS1 Style, WS1000 Connect, Solexa II and control units Remo 8, Remo pro, RF-B2-UP, Corlo P RF. Output for dimmable LED in combination with dimmable power supply units. Radio frequency 868.2 MHz (Elsner RF).
Connector housing STAK3/STAS3, dimensions approx. 147 x 36 x 29 (W x H x D, mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 60545 RF-L LED-ST IP53

Wireless dimmer RF-L LED-ST IP54

Wireless dimmer for 1 consumer for controllers WS1000 Colour, KNX WS1000 Colour, WS1 Colour, WS1000 Style, KNX WS1000 Style, WS1 Style, WS1000 Connect, Solexa II and control units Remo 8, Remo pro, RF-B2-UP, Corlo P RF. Output for dimmable LED in combination with dimmable power supply units. Radio frequency 868.2 MHz (Elsner RF).
Connector housing STAK3/STAS3, dimensions approx. 147 x 49 x 32 (W x H x D, mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 60557 RF-L LED-ST IP54

Wireless dimmer RF-L-UP 1-10V

Wireless dimmer and switch for 1 consumer for controllers WS1000 Colour, KNX WS1000 Colour, WS1 Colour, WS1000 Style, KNX WS1000 Style, WS1 Style, WS1000 Connect, Solexa II and control units Remo 8, Remo pro, RF-B2-UP, Corlo P RF. Switch output, control interface 1-10 V for electronic enhanced voltage generators (EVG), LED converters, electronic power supply units for low-voltage systems. Radio frequency 868.2 MHz (Elsner RF).
Built-in device, dimensions 50 x 50 x 54 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 60547 RF-L-UP 1-10V