KNX W 12…40 V DC / 12...28 V AC Wind Sensor invitation to tender

Wind sensor for the KNX bus system. Detection of the wind speed. Operating voltage 12…40 V DC / 12...28 V AC. Application with 3 wind threshold values, 8 AND logic gates and 8 OR logic gates. 80 communication objects. 
Including combi-mount for wall/mast mounting. Dimensions 96 x 77 x 118 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70123 KNX W 12…40 V DC / 12...28 V AC

KNX W sl Wind Sensor invitation to tender

Wind sensor for the KNX bus system. Detection of the wind speed. Operating voltage 12…40 V DC / 12...28 V AC. Application with 4 wind threshold values, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 176 communication objects. 
For wall/mast mounting. Dimensions 62 x 71 x 145 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70158 KNX W sl

KNX L Brightness Sensor invitation to tender

Brightness sensor for the KNX bus system. Operating voltage KNX bus voltage. Application with 3 brightness threshold values for daytime, 3 twilight threshold values for night-time, 8 AND logic gates and 8 OR logic gates. 117 communication objects. 
Including combi-mount for wall/mast mounting. Dimensions 96 x 77 x 118 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70119 KNX L

KNX LW 12…40 V DC / 12...28 V AC Brightness/Wind Sensor invitation to tender

Combi-sensor for the KNX bus system. Detection of the brightness and wind speed. Operating voltage 12…40 V DC / 12...28 V AC. Application with 3 wind threshold values, 3 brightness threshold values for daytime, 3 twilight threshold values for night-time, 8 AND logic gates and 8 OR logic gates. 117 communication objects. 
Including combi-mount for wall/mast mounting. Dimensions 96 x 77 x 118 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70129 KNX LW 12…40 V DC / 12...28 V AC

KNX LW sl Brightness/Wind Sensor invitation to tender

Combi-sensor for the KNX bus system. Detection of the brightness and wind speed. Operating voltage 12…40 V DC / 12...28 V AC. Application with 4 wind threshold values, 4 brightness threshold values for daytime, 4 twilight threshold values for night-time, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 303 communication objects. 
For wall/mast mounting. Dimensions 62 x 71 x 145 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70164 KNX LW sl

KNX RW 24 V DC Rain/Wind Sensor invitation to tender

Combi-sensor for the KNX bus system. Detection of precipitation and wind speed. Operating voltage 24 V DC. Application with 3 wind threshold values, 1 rain switching output, 8 AND logic gates and 8 OR logic gates. 81 communication objects. 
Including combi-mount for wall/mast mounting. Dimensions 96 x 77 x 118 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70127 KNX RW 24 V DC

KNX RW sl Rain/Wind Sensor invitation to tender

Combi-sensor for the KNX bus system. Detection of precipitation and wind speed. Operating voltage 12…40 V DC / 12...28 V AC. Application with 4 wind threshold values, 1 rain switching output, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 182 communication objects. 
For wall/mast mounting. Dimensions 62 x 71 x 145 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70162 KNX RW sl