Title: An Firma
Author: MD
Last saved by: Hagenlocher, Joachim

KNX CP TP Area and Line Coupler

Interface between two KNX TP lines (main and subline). Use as line coupler, area coupler or as repeater (without filtering). Routing filter for group and individual telegrams (incl. button for temporary deactivation), supports long telegrams. Suppression of configuration from subline to main line. Functions for troubleshooting, fast commissioning and avoidance of unnecessary telegram traffic. Multi-coloured LEDs display status information.
Modular device for mounting on top-hat rail according to DIN EN 60715. Dimensions 36 x 90 x 71 (W x H x D in mm), 2 division units.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70148 KNX CP TP

Elsner Elektronik GmbH | Sohlengrund 16 | 75395 Ostelsheim | www.elsner-elektronik.de	

Stand 31.08.2021