KNX PY global irradiance sensor invitation to tender

Pyranometer for measuring of global irradiance for the KNX bus system. 4 threshold values. 2 AND and 2 OR logic gates. 52 communication objects. Operating voltage: bus voltage.
Including combi-mount for wall/mast mounting. Dimensions 96 x 77 x 118 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX PY global irradiance sensor