KNX T-UN 100 Temperature Sensor invitation to tender

Temperature sensor for the KNX bus system. Evaluation unit with T-100 feed/contact probe. 
Application with calculation of mixed values, 4 temperature threshold values, temperature PI controller, 4 AND logic gates and 4 OR logic gates.
80 communication objects. Operating voltage: KNX bus voltage.
Evaluation unit: Mounting in junction box, dimensions 38 x 47 x 24 (W x H x D, mm).
Probe: Protection category IP 43, measurement range -35…+100°C, length of sensor sleeve approx. 32 mm, diameter approx. 6 mm, cable length approx. 300 cm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70221 KNX T-UN 100

KNX T-UN 130 Temperature Sensor invitation to tender

Temperature sensor for the KNX bus system. Evaluation unit with T-100 feed/contact probe. 
Application with calculation of mixed values, 4 temperature threshold values, temperature PI controller, 4 AND logic gates and 4 OR logic gates.
80 communication objects. Operating voltage: KNX bus voltage.
Evaluation unit: Mounting in junction box, dimensions 38 x 47 x 24 (W x H x D, mm).
Probe: Protection category IP 68, measurement range -30…+130°C, length of sensor sleeve approx. 20 mm, diameter approx. 6 mm, cable length approx. 300 cm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70220 KNX T-UN 130