Brightness Sensor Vari KNX 3L invitation to tender

Sensor for the KNX bus system for indoor and outdoor applications. Recording of brightness (3 sensors). 
Switching outputs depending on limit values. 8 AND and 8 OR logic gates. 8 multifunctional modules for calculation, conditions, transition. 
274 communication objects. 
Integrated mount for wall/mast mounting. Dimensions 65 x 80 x 30 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Typ: 70382 Vari KNX 3L

Combined Sensor Vari KNX 3L-T invitation to tender

Sensor for the KNX bus system for indoor and outdoor applications. Recording of brightness (3 sensors) and temperature. 
Switching outputs depending on limit values. PI control for heating/cooling depending on temperature. Summer compensation for cooling. 
8 AND and 8 OR logic gates. 8 multifunctional modules for calculation, conditions, transition. 
339 communication objects. 
Integrated mount for wall/mast mounting. Dimensions 65 x 80 x 30 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Typ: 70383 Vari KNX 3L-T

Combined Sensor Vari KNX 3L-TH invitation to tender

Sensor for the KNX bus system for indoor and outdoor applications. Recording of brightness (3 sensors), temperature and air humidity. 
Switching outputs depending on limit values. PI control for heating/cooling depending on temperature and PI control for (de-)humidification depending on humidity. Summer compensation for cooling. 4 actuating variable comparators.
8 AND and 8 OR logic gates. 8 multifunctional modules for calculation, conditions, transition. 
421 communication objects. 
Integrated mount for wall/mast mounting. Dimensions 65 x 80 x 30 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Typ: 70384 Vari KNX 3L-TH

Temperature Sensor Vari KNX T invitation to tender

Sensor for the KNX bus system for indoor and outdoor applications. Recording of temperature. 
Switching outputs depending on limit values. PI control for heating/cooling depending on temperature. Summer compensation for cooling.
8 AND and 8 OR logic gates. 8 multifunctional modules for calculation, conditions, transition. 
212 communication objects. 
Integrated mount for wall/mast mounting. Dimensions 65 x 80 x 30 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Typ: 70385 Vari KNX T

Combined Sensor Vari KNX TH invitation to tender

Sensor for the KNX bus system for indoor and outdoor applications. Recording of temperature and air humidity.
Switching outputs depending on limit values. Calculation of the dewpoint, monitoring of the comfort field according to DIN 1946. PI control for heating/cooling depending on temperature and PI control for (de-)humidification depending on humidity. Summer compensation for cooling. 4 actuating variable comparators.
8 AND and 8 OR logic gates. 8 multifunctional modules for calculation, conditions, transition. 
294 communication objects. 
Integrated mount for wall/mast mounting. Dimensions 65 x 80 x 30 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Typ: 70386 Vari KNX TH

GPS Receiver Vari KNX GPS invitation to tender

GPS receiver for the KNX bus system. Output of time and position coordinates. Calculation of the position of the sun. Calendar and week time switch. 
150 communication objects. 
Integrated mount for wall/mast mounting. Dimensions 65 x 80 x 30 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Typ: 70387 Vari KNX GPS

Combined Sensor Vari KNX TH-D invitation to tender

Sensor for the KNX bus system for indoor and outdoor applications. Recording of temperature, air humidity and air pressure.
Switching outputs depending on limit values. Calculation of the dewpoint, monitoring of the comfort field according to DIN 1946. PI control for heating/cooling depending on temperature and PI control for (de-)humidification depending on humidity. Summer compensation for cooling. 4 actuating variable comparators.
8 AND and 8 OR logic gates. 8 multifunctional modules for calculation, conditions, transition. 
328 communication objects. 
Integrated mount for wall/mast mounting. Dimensions 65 x 80 x 30 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Typ: 70388 Vari KNX TH-D

Combined Sensor Vari KNX 3L-TH-D invitation to tender

Sensor for the KNX bus system for indoor and outdoor applications. Recording of brightness (3 sensors), temperature, air humidity and air pressure.
Switching outputs depending on limit values. Calculation of the dewpoint, monitoring of the comfort field according to DIN 1946. PI control for heating/cooling depending on temperature and PI control for (de-)humidification depending on humidity. Summer compensation for cooling. 4 actuating variable comparators.
8 AND and 8 OR logic gates. 8 multifunctional modules for calculation, conditions, transition. 
455 communication objects. 
Integrated mount for wall/mast mounting. Dimensions 65 x 80 x 30 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Typ: 70389 Vari KNX 3L-TH-D

Combined Sensor Vari KNX 3L-TH-D-GPS invitation to tender

Sensor for the KNX bus system for indoor and outdoor applications. Recording of brightness (3 sensors), temperature, air humidity and air pressure. With GPS receiver.
Switching outputs depending on limit values. Calculation of the dewpoint, monitoring of the comfort field according to DIN 1946. PI control for heating/cooling depending on temperature and PI control for (de-)humidification depending on humidity. Summer compensation for cooling. 4 actuating variable comparators. 
Output of time and position coordinates. Calculation of the position of the sun. Calendar and week time switch. 
8 AND and 8 OR logic gates. 8 multifunctional modules for calculation, conditions, transition. 
603 communication objects. 
Integrated mount for wall/mast mounting. Dimensions 65 x 80 x 30 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Typ: 70390 Vari KNX 3L-TH-D-GPS