Corlo Touch KNX 5in invitation to tender

Touch switch, controller and info display for KNX. 5" colour touch display. 10 pages for operation and display. RGB frame illumination. Integrated proximity and brightness sensors. Integrated automatic functions for shading (sun/eye protection) and ambient climate control (heating, cooling, exhaust air extraction). Setting via ETS, adjustment at the display is possible.
KNX connection for data transfer. 4 inputs for binary contacts or temperature sensor. Micro SD card plug-in socket.
Operating voltage: 24 V DC ±10%. Dimensions 133 x 97 x 35 (W x H x D in mm). Colour black, integrated frame black. Mounting on a socket.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70481 Corlo Touch KNX 5in

Corlo Touch KNX 5in WL invitation to tender

Touch switch, controller and info display for KNX. 5" colour touch display. 10 pages for operation and display. RGB frame illumination. Integrated proximity and brightness sensors. Integrated automatic functions for shading (sun/eye protection) and ambient climate control (heating, cooling, exhaust air extraction). Setting via ETS, adjustment at the display is possible.
KNX connection for data transfer. WLAN interface for communication with Corlo Mobile App and for display of web pages, visualisations, IP camera pictures. 4 inputs for binary contacts or temperature sensor. Micro SD card plug-in socket.
Operating voltage: 24 V DC ±10%. Dimensions 133 x 97 x 35 (W x H x D in mm). Colour black, integrated frame black. Mounting on a socket.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70475 Corlo Touch KNX 5in WL

T-NTC Temperature Sensor invitation to tender

Temperature feed/contact probe. Protection category IP 43. Measurement range -35…+100°C. Length of sensor sleeve approx. 32 mm, diameter approx. 6 mm, cable length approx. 300 cm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 30516 T-NTC