KNX TH-UP Touch CH Indoor Sensor, pure white RAL 9010

Indoor sensor for the KNX bus system. Measuring of temperature and air humidity (relative, absolute). Calculation of the dew point. Calculation of mixed values. 5 threshold values. Logic links (AND and OR). Integrated PI controller for heating/cooling (temperature) and for one- or two-step ventilation (humidity). Variable comparators. 186 communication objects. Operating voltage: KNX bus voltage.
With display and touch buttons (keys for target value change, mode change or as bus push-buttons).
Wall installation, flush-mounted in inlet box. Mounting with 2 spring clips in mounting adapter. For use in Swiss switch system with frame size 60 mm, supplied without frame. Colour: white.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70637 KNX TH-UP Touch CH, pure white RAL 9010

KNX TH-UP Touch CH Indoor Sensor, deep black RAL 9005

Indoor sensor for the KNX bus system. Measuring of temperature and air humidity (relative, absolute). Calculation of the dew point. Calculation of mixed values. 5 threshold values. Logic links (AND and OR). Integrated PI controller for heating/cooling (temperature) and for one- or two-step ventilation (humidity). Variable comparators. 186 communication objects. Operating voltage: KNX bus voltage.
With display and touch buttons (keys for target value change, mode change or as bus push-buttons).
Wall installation, flush-mounted in inlet box. Mounting with 2 spring clips in mounting adapter. For use in Swiss switch system with frame size 60 mm, supplied without frame. Colour: black.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70638 KNX TH-UP Touch CH, deep black RAL 9005