KNX VOC/TH-UP Touch Indoor Sensor pure white

Indoor sensor for the KNX bus system. Measuring of VOC (volatile organic compounds), temperature and air humidity (relative, absolute). Calculation of the dew point. Calculation of mixed values. 9 threshold values. Logic links (AND and OR). Integrated PI controller for heating/cooling (temperature) and for one- or two-step ventilation (humidity/VOC). Variable comparators. 224 communication objects. Operating voltage: KNX bus voltage.
With display and touch buttons (keys for target value change, mode change or as bus push-buttons). Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W xH in mm), installation depth approx. 8 mm Base plate dimensions: approx. 71 x 71 (W x H in mm). Colour: RAL 9010 pure white.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70970 KNX VOC/TH-UP Touch white

KNX VOC/TH-UP Touch Indoor Sensor jet black

Indoor sensor for the KNX bus system. Measuring of VOC (volatile organic compounds), temperature and air humidity (relative, absolute). Calculation of the dew point. Calculation of mixed values. 9 threshold values. Logic links (AND and OR). Integrated PI controller for heating/cooling (temperature) and for one- or two-step ventilation (humidity/VOC). Variable comparators. 224 communication objects. Operating voltage: KNX bus voltage.
With display and touch buttons (keys for target value change, mode change or as bus push-buttons). Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W xH in mm), installation depth approx. 8 mm Base plate dimensions: approx. 71 x 71 (W x H in mm). Colour: RAL 9005 jet black.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70973 KNX VOC/TH-UP Touch black