Cala KNX T 101 Temperature Controller, pure white RAL 9010

Room temperature controller for the KNX bus system. Measuring of temperature. Calculation of mixed value. Integrated PI controller for one- or two-step heating/cooling. 41 communication objects. 
With temperature display (measured value, target value or basic setpoint shift) and touch buttons for manual adjustment of the room temperature. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: pure white RAL 9010.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70980 Cala KNX T 101, pure white RAL 9010

Cala KNX T 101 Temperature Controller, jet black RAL 9005

Room temperature controller for the KNX bus system. Measuring of temperature. Calculation of mixed value. Integrated PI controller for one- or two-step heating/cooling. 41 communication objects. 
With temperature display (measured value, target value or basic setpoint shift) and touch buttons for manual adjustment of the room temperature. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70982 Cala KNX T 101, jet black RAL 9005