Cala KNX T 201 Sunblind push button, pure white RAL 9010

Push button with temperature sensor for the KNX bus system. With temperature display (measured value, target value or basic setpoint shift) and 4 touch buttons (bus push buttons), divided into 2 areas, printed with icons for the functions:
•	Temperature control (warmer, cooler) with configurable LEDs (switch via objects)
•	Drive (up/down with distinction short/long) ) with configurable LEDs (switch via objects).
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. PI controller for heating/cooling (by temperature). 92 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: pure white RAL 9010.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70990 Cala KNX T 201 Sunblind, pure white RAL 9010

Cala KNX T 201 Sunblind push button, jet black RAL 9005

Push button with temperature sensor for the KNX bus system. With temperature display (measured value, target value or basic setpoint shift) and 4 touch buttons (bus push buttons), divided into 2 areas, printed with icons for the functions:
•	Temperature control (warmer, cooler) with configurable LEDs (switch via objects)
•	Drive (up/down with distinction short/long) ) with configurable LEDs (switch via objects).
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. PI controller for heating/cooling (by temperature). 92 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70992 Cala KNX T 201 Sunblind, jet black RAL 9005

Cala KNX T 202 Sunblind push button, pure white RAL 9010

Push button with temperature sensor for the KNX bus system. With temperature display (measured value, target value or basic setpoint shift) and 6 touch buttons (bus push buttons), divided into 3 areas, printed with icons for the functions:
•	Temperature control (warmer, cooler) with configurable LEDs (switch via objects)
•	2 areas for drives (up/down with distinction short/long) ) with configurable LEDs (switch via objects).
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. PI controller for heating/cooling (by temperature). 98 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: pure white RAL 9010.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71050 Cala KNX T 202 Sunblind, pure white RAL 9010

Cala KNX T 202 Sunblind push button, jet black RAL 9005

Push button with temperature sensor for the KNX bus system. With temperature display (measured value, target value or basic setpoint shift) and 6 touch buttons (bus push buttons), divided into 3 areas, printed with icons for the functions:
•	Temperature control (warmer, cooler) with configurable LEDs (switch via objects)
•	2 areas for drives (up/down with distinction short/long) ) with configurable LEDs (switch via objects).
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. PI controller for heating/cooling (by temperature). 98 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71052 Cala KNX T 202 Sunblind, jet black RAL 9005