KNX eTR M1 push button, signal white RAL 9003

1-gang push button with temperature sensor for the KNX bus system. With 1 touch button (bus push button) and 1 configurable LED (switching via objects).
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 44 communication objects. 
Glass surface. Wall installation with or without equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: signal white RAL 9003.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71110 KNX eTR M1, signal white RAL 9003

KNX eTR M1 push button, jet black RAL 9005

1-gang push button with temperature sensor for the KNX bus system. With 1 touch button (bus push button) and 1 configurable LED (switching via objects).
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 44 communication objects. 
Glass surface. Wall installation with or without equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71112 KNX eTR M1, jet black RAL 9005

KNX eTR M2 push button, signal white RAL 9003

2-gang push button with temperature sensor for the KNX bus system. With 2 touch button (bus push button) and 2 configurable LED (switching via objects). Area function by touching multiple keys.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 55 communication objects. 
Glass surface. Wall installation with or without equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: signal white RAL 9003.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71120 KNX eTR M2, signal white RAL 9003

KNX eTR M2 push button, jet black RAL 9005

2-gang push button with temperature sensor for the KNX bus system. With 2 touch button (bus push button) and 2 configurable LED (switching via objects). Area function by touching multiple keys.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 55 communication objects. 
Glass surface. Wall installation with or without equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71122 KNX eTR M2, jet black RAL 9005

KNX eTR M4 push button, signal white RAL 9003

4-gang push button with temperature sensor for the KNX bus system. With 4 touch button (bus push button) and 4 configurable LED (switching via objects). Area function by touching multiple keys.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 73 communication objects. 
Glass surface. Wall installation with or without equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: signal white RAL 9003.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71130 KNX eTR M4, signal white RAL 9003

KNX eTR M4 push button, jet black RAL 9005

4-gang push button with temperature sensor for the KNX bus system. With 4 touch button (bus push button) and 4 configurable LED (switching via objects). Area function by touching multiple keys.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 73 communication objects. 
Glass surface. Wall installation with or without equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71132 KNX eTR M4, jet black RAL 9005