KNX eTR 208 Light/Sunblind push button, signal white RAL 9003

Touch push button with temperature sensor for the KNX bus system. With temperature display (measured value, target value or basic setpoint shift) and 6 touch buttons (bus push buttons), divided into 3 areas, printed with icons for the functions:
•	Temperature controller (setpoint adjuster, changeover heating controller/cooling controller) with configurable LEDs (switch via objects)
•	Light switch (switching and dimming) with configurable LED (switching via objects)
•	Drive (up/down with distinction short/long) with configurable LEDs (switch via objects).
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. PI controller for heating/cooling (by temperature). 98 communication objects. 
Glass surface. Wall installation with or without equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: signal white RAL 9003.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71190 KNX eTR 208 Light/Sunblind, signal white RAL 9003

KNX eTR 208 Light/Sunblind push button, jet black RAL 9005

Touch push button with temperature sensor for the KNX bus system. With temperature display (measured value, target value or basic setpoint shift) and 6 touch buttons (bus push buttons), divided into 3 areas, printed with icons for the functions:
•	Temperature controller (setpoint adjuster, changeover heating controller/cooling controller) with configurable LEDs (switch via objects)
•	Light switch (switching and dimming) with configurable LED (switching via objects)
•	Drive (up/down with distinction short/long) with configurable LEDs (switch via objects).
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. PI controller for heating/cooling (by temperature). 98 communication objects. 
Glass surface. Wall installation with or without equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71192 KNX eTR 208 Light/Sunblind, jet black RAL 9005