KNX eTR 101-BA2 Room Temperature Controller with 2 A/D Inputs, signal white RAL 9003

Room temperature controller for the KNX bus system. Measuring of temperature. Calculation of mixed value. Integrated PI controller for one- or two-step heating/cooling. 77 communication objects. Operating voltage: KNX bus voltage. 2 inputs (binary inputs or for temperature sensor T-NTC, no. 30516).
With temperature display (measured value, target value or basic setpoint shift) and touch buttons for manual adjustment of the room temperature. Wall installation with equipment socket. Colour RAL 9003 signal white. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71310 KNX eTR 101-BA2, signal white RAL 9003

KNX eTR 101-BA2 Room Temperature Controller with 2 A/D Inputs, jet black RAL 9005

Room temperature controller for the KNX bus system. Measuring of temperature. Calculation of mixed value. Integrated PI controller for one- or two-step heating/cooling. 77 communication objects. Operating voltage: KNX bus voltage. 2 inputs (binary inputs or for temperature sensor T-NTC, no. 30516).
With temperature display (measured value, target value or basic setpoint shift) and touch buttons for manual adjustment of the room temperature. Wall installation with equipment socket. Colour RAL 9005 jet black. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71312 KNX eTR 101-BA2, jet black RAL 9005