Switch for Room Service KNX eTR DND/MUR Switch, signal white RAL 9003

Switch with temperature sensor for the KNX bus system, specially developed for the GRMS (Guest Room Management System) of hotels. Guest can choose between:
•	Do Not Disturb (DND)
•	Make Up Room (MUR)
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 67 communication objects. 
Glass surface. Wall installation with equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: signal white RAL 9003.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71330 KNX eTR DND/MUR Switch, signal white RAL 9003

Switch for Room Service KNX eTR DND/MUR Switch, jet black RAL 9005

Switch with temperature sensor for the KNX bus system, specially developed for the GRMS (Guest Room Management System) of hotels. Guest can choose between:
•	Do Not Disturb (DND)
•	Make Up Room (MUR)
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 67 communication objects. 
Glass surface. Wall installation with equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71332 KNX eTR DND/MUR Switch, jet black RAL 9005

Signal for Room Service and Doorbell KNX eTR DND/MUR Signal/Bell, signal white RAL 9003

Signal with temperature sensor for the KNX bus system, specially developed for the GRMS (Guest Room Management System) of hotels. Device shows the guest's service selection:
•	Do Not Disturb (DND)
•	Make Up Room (MUR)
Touch surface with bell symbol for use as a bell.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 67 communication objects. 
Glass surface. Wall installation with equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: signal white RAL 9003.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71334 KNX eTR DND/MUR Signal/Bell, signal white RAL 9003

Signal for Room Service and Doorbell KNX eTR DND/MUR Signal/Bell, jet black RAL 9005

Signal with temperature sensor for the KNX bus system, specially developed for the GRMS (Guest Room Management System) of hotels. Device shows the guest's service selection:
•	Do Not Disturb (DND)
•	Make Up Room (MUR)
Touch surface with bell symbol for use as a bell.
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 67 communication objects. 
Glass surface. Wall installation with equipment socket. Housing dimensions: approx. 81,5 x 81,5 (W x H in mm), installation depth approx. 12 mm. Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 71336 KNX eTR DND/MUR Signal/Bell, jet black RAL 9005