# Glastaster für Hotels

Die Taster **KNX eTR DND/MUR Switch** und **KNX eTR DND/MUR Signal/Bell** ermöglichen eine komfortable und effiziente Kommunikation zwischen Gast und Hotelpersonal – vollständig integriert in KNX.

KNX eTR DND/MUR Switch wird im Hotelzimmer installiert und dient der Auswahl des gewünschten Servicezustands: „Bitte nicht stören“ oder „Zimmer reinigen“. Die Touch-Glasoberfläche mit hinterleuchteten Icons ermöglicht eine intuitive Bedienung. Der gewählte Status kann im System genutzt und an der Gegenstelle im Flur angezeigt werden. Zusätzlich ist im KNX eTR DND/MUR Signal/Bell eine Zimmer-Klingel integriert. Beide Geräte sind Teil der Serie **eTR** und lassen sich mit weiteren Tastern und Raumreglern kombinieren.

# Glass Buttons for Hotels

The KNX eTR DND/MUR Switch and KNX eTR DND/MUR Signal/Bell buttons enable convenient and efficient communication between guests and hotel staff – fully integrated into KNX.

The KNX eTR DND/MUR Switch is installed in the hotel room and is used to select the desired service status: "Do Not Disturb" or "Make Up Room". The touch glass surface with backlit icons enables intuitive operation. The selected status can be used in the system and displayed at the counterpart button in the corridor. In addition, a room bell is integrated into the KNX eTR DND/MUR Signal/Bell. Both devices are part of the eTR series and can be combined with other push buttons and room controllers.