KNX-GPS Suntracer weather station invitation to tender

Weather station for the KNX bus system. Recording of brightness, wind speed, precipitation (heated sensor), temperature. Calculation of the sun's position. GPS receiver (time, date, position), calendar and week timer. Integrated shading control, shadow edge and lamella tracking for 6 façades. 8 AND and 8 OR logic gates. 254 communication objects. Operating volatge 12-40 V DC (12-28 V AC).
Including combi-mount for wall/mast mounting. Dimensions 96 x 77 x 118 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 3093 Suntracer KNX-GPS