Title: An Firma
Author: MD
Last saved by: Buse, Rita

Wireless dimmer RF-L-DST 1-10 V

Wireless dimmer for 1 consumer for controllers WS1000 Colour, KNX WS1000 Colour, WS1 Colour, WS1000 Style, KNX WS1000 Style, WS1 Style, Solexa II and control units Remo 8, Remo pro, RF-B2-UP, Corlo P RF. For lights with electronic enhaced voltage generator (EVG), LED converter or electronic power supply for low voltage systems. 230 V switched output (16 A) and 1-10 V control output. Radio frequency 868.2 MHz (Elsner RF).
Connector housing STAK3/STAS3, dimensions approx. 149 x 72 x 29 (W x H x D, mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 60561 RF-L-DST 1-10 V

Wireless dimmer RF-L-DST DALI

Wireless dimmer for 1 consumer for controllers WS1000 Colour, KNX WS1000 Colour, WS1 Colour, WS1000 Style, KNX WS1000 Style, WS1 Style, Solexa II and control units Remo 8, Remo pro, RF-B2-UP, Corlo P RF. DALI control for lights with switching power supplies, electronic enhaced voltage generator (EVG) or electronic power supplys. 230 V switched output (16 A) and DALI control output (broadcast operation). Radio frequency 868.2 MHz (Elsner RF).
Connector housing STAK3/STAS3, dimensions approx. 149 x 72 x 29 (W x H x D, mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 60562 RF-L-DST DALI

Elsner Elektronik GmbH | Sohlengrund 16 | 75395 Ostelsheim | www.elsner-elektronik.de	

Version: 20/12/2018